

|  |
| --- |
| REQUEST FOR TENDER |
| Construction of Concrete Road, Driveways, and Stormwater Drainage at the Green St, Georgetown Staff Housing Facility |
| CONTRACT NO: ESC2024-047 |

Request for Tender

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **PART 1 – PREAMBLE** | | | | | |
| Etheridge Shire Council invites tenders from suitably qualified tenderers for the Construction of Concrete Road, Driveways, and Stormwater Drainage at the Green St, Georgetown Staff Housing Facility | | | | | |
| **PART 2 – GENERAL INFORMATION** | | | | | |
| 1. Contract details: | ESC2024-047 | | | | |
| 2. Communications by Tenderers: | All communications related to Tender must be submitted to [tender@etheridge.qld.gov.a](mailto:tender@etheridge.qld.gov.au)u. | | | | |
| 3. Briefing or site inspection: | Details | Maximum attendees | Mandatory | RSVP | |
| The project location at the new staff housing Facility at Green Street, Georgetown | NA | NA | Tenderers must inform Council and give notice as works are currently in progress. | |
| 4. Submission of Tender: | Tenders must be submitted by email to [tender@etheridge.qld.gov.au](mailto:tender@etheridge.qld.gov.au) by no later than 12:00 PM on 6th January 2025. | | | | |
| 5. Evaluation Criteria: | Evaluation Criteria | | | | Weighting (%) (Optional) |
| Capability and Experience | | | | 20 |
| Delivery Timeframe | | | | 10 |
| Local Preference | | | | 10 |
| Value for Money | | | | 40 |
| Quality, Safety, Environment Management Systems | | | | 20 |
| 6. Tenders to be valid for: | 90 calendar days after the time stated in Item 4 (as extended if at all, pursuant to the Procurement Process Conditions) | | | | |
| 7. Complaints: | Complaints regarding Procurement Process to be directed to [tender@etheridge.qld.gov.au](mailto:tender@etheridge.qld.gov.au) | | | | |
| **PART 3 – PROCUREMENT PROCESS CONDITIONS** | | | | | |
| The Procurement Process is governed by, and this Request for Tender is to be read in conjunction with, the Procurement Process Conditions attached to or provided with this Request for Tender and identified as Procurement- Process-Conditions. | | | | | |
| **PART 4 – CONTRACT** | | | | | |
| The contract is scheduled for rates and shall be substantially in the form attached to or provided with this Request for Tender and identified as Contract-Construct-Only-Standard-Risk. | | | | | |
| **PART 5 – SCOPE** | | | | | |
| The project involves site establishment, excavation, and disposal of unsuitable materials. It includes construction of 32 MPa concrete roads, parking areas, driveways, Concrete invert, and laybacks with appropriate formwork and reinforcement. It includes laying and compacting crushed dust for pavement. Stormwater drainage works include installing PVC pipes, kerb inlet pits, and inlet pits. All works must comply with Etheridge Shire Council specifications, incorporating environmental management, OH&S standards, and preparation of Work-As-Executed (WAE) drawings to ensure quality and adherence to standards. | | | | | |
| **PART 6 – RESPONSE SCHEDULES** | | | | | |
| The Tender must be submitted in the form provided in the response schedules attached to or provided with this  Request for Tender and identified as Response-Schedule-Works. | | | | | |

Request for Tender (Generic) Issue: LGT2.0

Effective Date: July 2023 Page | 1